Author: martijn.dejongh

STERN TRAWLER

NVC 376 WP

NVC 376 WP
85M STERN TRAWLER FOR ARCTIC WATERS
General
Our family of trawlers are all designed for safe, environmentally friendly, reliable and economical fishing in harsh and ice infected waters.
The stern trawler vessels may be fitted with different propulsion systems; single-screw, twin screw, azimuthing thruster in foreship. Depending on operational profile of vessel, we will, in close cooperation with Owners, find the optimal propulsion system for each specific vessel and fishing operation.

CLASS
Any IACS Class Society
Polar Code Compliant-Ice class
Main Features
Length overall approx. 84,90 m
Breadth, mld approx. 18,00 m
Draught, design approx. 7,00 m
Draught, summer/Scantling approx. 7,50 m
ACCOMMODATION
Accommodation and equipment for 25 persons, 25 cabins.
HOLD CAPACITY
Freezing Holds (Tween deck) appr.2000 m3
Packing/Freezing Holds appr. 450 m3
Ensilage appr. 540 m3
FISHING SYSTEM
Single, Double or Triple trawling.
PROCESSING
Higly effectice processing for white fish, H/G or fillet. Shrimp, cooked and industrial up to 120 tons/day.
Ensilage plant

SHIP DESIGN AND INTEGRATED SYSTEMS

DESIGN AND
INTEGRATED SYSTEMS
Ship Design Solutions can provide Ship Design alone or integrated system solutions for:
Propulsion systems
Winches deck systems
Energy Storage systems
Power generation systems
Integrated Automation systems
Integrated Bridge solutions

Web page:

https://www.kongsberg.com/maritime/shipdesign

E-mail:

smb632.ship.design@km.kongsberg.com