Author: martijn.dejongh

STERN TRAWLER

NVC 370 WP

NVC 370 WP
70 M STERN TRAWLER
General
Our family of trawlers are all designed for safe, environmentally friendly, reliable and economical fishing in harsh waters.
The stern trawler vessels may be fitted with different propulsion systems; single-screw, twin screw, azimuthing thruster in foreship. Depending on operational profile of vessel, we will, in close cooperation with Owners, find the optimal propulsion system for each specific vessel and fishing operation.

CLASS
Any IACS Class Society
High Ice class
Main Features
Length overall approx. 69,90 m
Breadth, moulded approx. 16,00 m
Draught, design approx. 6,00 m
Draught, summer/Scantling approx. 6,70 m
ACCOMMODATION
Accommodation and equipment for 29 persons, 22 cabins.
HOLD CAPACITY
Freezing Holds appr.1300 m3
Ensilage appr. 280 m3
Packing Hold appr. 250 m3
FISHING SYSTEM
Single, Double or Triple trawling.
PROCESSING
Higly effective processing for white fish and shrimp up to 80 tons/day.
Ensilage processing plant.

SHIP DESIGN AND INTEGRATED SYSTEMS

DESIGN AND
INTEGRATED SYSTEMS
Ship Design Solutions can provide Ship Design alone or integrated system solutions for:
Propulsion systems
Winches deck systems
Energy Storage systems
Power generation systems
Integrated Automation systems
Integrated Bridge solutions

Web page:

https://www.kongsberg.com/maritime/shipdesign

E-mail:

smb632.ship.design@km.kongsberg.com