| EM datagrams on *.kmall format Reg. nr. 410224 rev I

Data Fields
EMdgmSCLdataFromSensor_def Struct Reference

Part of clock datagram giving offsets and the raw input in text format. More...

`#include <EMdgmFormat.h>`

## Data Fields
float | offset_sec
int32_t | clockDevPU_microsec
uint8_t | dataFromSensor [MAX_SCL_DATALENGTH]

## Detailed Description

Part of clock datagram giving offsets and the raw input in text format.

Definition at line 573 of file EMdgmFormat.h.

## Field Documentation

## ◆ offset_sec

float offset_sec

Offset in seconds from K-Controller operator input.

Definition at line 577 of file EMdgmFormat.h.

## ◆ clockDevPU_microsec

int32_t clockDevPU_microsec

Clock deviation from PU. Difference between time stamp at receive of sensor data and time in the clock source. Unit microseconds. Difference smaller than +/- 1 second if 1PPS is active and sync from ZDA.

Definition at line 578 of file EMdgmFormat.h.

## ◆ dataFromSensor

uint8_t dataFromSensor[MAX_SCL_DATALENGTH]

Clock data as received from sensor, in text format. Data are uncorrected for offsets.

Definition at line 581 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h