| EM datagrams on *.kmall format Reg.no. 410224 rev F

Data Fields
EMdgmCPO_def Struct Reference

#CPO - Struct of compatibility position sensor datagram.
Data from active sensor will be motion corrected if indicated by operator. Motion correction is applied to latitude, longitude, speed, course and ellipsoidal height. If the sensor is inactive, the fields will be marked as unavailable, defined by the parameters define UNAVAILABLE_LATITUDE etc. More...

`#include <EMdgmFormat.h>`

Collaboration diagram for EMdgmCPO_def:
[legend]

## Data Fields
struct EMdgmHeader_def | header
struct EMdgmScommon_def | cmnPart
struct EMdgmCPOdataBlock_def | sensorData

## Detailed Description

#CPO - Struct of compatibility position sensor datagram.
Data from active sensor will be motion corrected if indicated by operator. Motion correction is applied to latitude, longitude, speed, course and ellipsoidal height. If the sensor is inactive, the fields will be marked as unavailable, defined by the parameters define UNAVAILABLE_LATITUDE etc.

Definition at line 1226 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h