| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmSdataInfo_def Struct Reference

Information of repeated sensor data in one datagram. More...

`#include <EMdgmFormat.h>`

## Data Fields
uint16_t | numBytesInfoPart
uint16_t | numSamplesArray
uint16_t | numBytesPerSample
uint16_t | numBytesRawSensorData

## Detailed Description

Information of repeated sensor data in one datagram.

Info about data from sensor. Part included if data from sensor appears multiple times in a datagram.

Definition at line 178 of file EMdgmFormat.h.

## Field Documentation

## ◆ numBytesInfoPart

uint16_t numBytesInfoPart

Size in bytes of current struct.

Definition at line 180 of file EMdgmFormat.h.

## ◆ numSamplesArray

uint16_t numSamplesArray

Number of sensor samples added in datagram.

Definition at line 181 of file EMdgmFormat.h.

## ◆ numBytesPerSample

uint16_t numBytesPerSample

Length in bytes of one whole sample (decoded and raw data).

Definition at line 182 of file EMdgmFormat.h.

## ◆ numBytesRawSensorData

uint16_t numBytesRawSensorData

Length in bytes of raw sensor data.

Definition at line 183 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h