| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmMWCtxSectorData_def Struct Reference

#MWC - data block 1: transmit sector data, loop for all i = numTxSectors. More...

`#include <EMdgmFormat.h>`

## Data Fields
float | tiltAngleReTx_deg
float | centreFreq_Hz
float | txBeamWidthAlong_deg
uint16_t | txSectorNum
int16_t | padding

## Detailed Description

#MWC - data block 1: transmit sector data, loop for all i = numTxSectors.

Definition at line 1111 of file EMdgmFormat.h.

## Field Documentation

## ◆ tiltAngleReTx_deg

float tiltAngleReTx_deg

Along ship steering angle of the TX beam (main lobe of transmitted pulse), angle referred to transducer face. Angle as used by beamformer (includes stabilisation). Unit degree.

Definition at line 1113 of file EMdgmFormat.h.

## ◆ centreFreq_Hz

float centreFreq_Hz

Centre frequency of current sector. Unit hertz.

Definition at line 1114 of file EMdgmFormat.h.

## ◆ txBeamWidthAlong_deg

float txBeamWidthAlong_deg

Corrected for frequency, sound velocity and tilt angle. Unit degree.

Definition at line 1115 of file EMdgmFormat.h.

## ◆ txSectorNum

uint16_t txSectorNum

Transmitting sector number.

Definition at line 1116 of file EMdgmFormat.h.

## ◆ padding

int16_t padding

Byte alignment.

Definition at line 1117 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h