| EM datagrams on *.kmall format Reg.no. 410224 rev F

Data Fields
EMdgmMWCtxInfo_def Struct Reference

#MWC - data block 1: transmit sectors, general info for all sectors More...

`#include <EMdgmFormat.h>`

## Data Fields
uint16_t | numBytesTxInfo
uint16_t | numTxSectors
uint16_t | numBytesPerTxSector
int16_t | padding
float | heave_m

## Detailed Description

#MWC - data block 1: transmit sectors, general info for all sectors

Definition at line 1089 of file EMdgmFormat.h.

## Field Documentation

## ◆ numBytesTxInfo

uint16_t numBytesTxInfo

Number of bytes in current struct.

Definition at line 1091 of file EMdgmFormat.h.

## ◆ numTxSectors

uint16_t numTxSectors

Number of transmitting sectors (Ntx). Denotes the number of times the struct EMdgmMWCtxSectorData is repeated in the datagram.

Definition at line 1092 of file EMdgmFormat.h.

## ◆ numBytesPerTxSector

uint16_t numBytesPerTxSector

Number of bytes in EMdgmMWCtxSectorData.

Definition at line 1094 of file EMdgmFormat.h.

## ◆ padding

int16_t padding

Byte alignment.

Definition at line 1095 of file EMdgmFormat.h.

## ◆ heave_m

float heave_m

Heave at vessel reference point, at time of ping, i.e. at midpoint of first tx pulse in rxfan.

Definition at line 1096 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h