| EM datagrams on *.kmall format Reg.no. 410224 rev E

Data Fields
EMdgmMWCtxSectorData_def Struct Reference

#MWC - data block 1: transmit sector data, loop for all i = numTxSectors. More...

`#include <EMdgmFormat.h>`

## Data Fields
float | tiltAngleReTx_deg
float | centreFreq_Hz
float | txBeamWidthAlong_deg
uint16_t | txSectorNum
int16_t | padding

## Detailed Description

#MWC - data block 1: transmit sector data, loop for all i = numTxSectors.

## Field Documentation

## ◆ tiltAngleReTx_deg

float tiltAngleReTx_deg

Along ship steering angle of the TX beam (main lobe of transmitted pulse), angle referred to transducer face. Angle as used by beamformer (includes stabilisation). Unit degree.

## ◆ centreFreq_Hz

float centreFreq_Hz

Centre frequency of current sector. Unit hertz.

## ◆ txBeamWidthAlong_deg

float txBeamWidthAlong_deg

Corrected for frequency, sound velocity and tilt angle. Unit degree.

## ◆ txSectorNum

uint16_t txSectorNum

Transmitting sector number.

## ◆ padding

int16_t padding

Byte alignment.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h