| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmSVPpoint_def Struct Reference

#SVP - Sound Velocity Profile. Data from one depth point contains information specified in this struct. More...

`#include <EMdgmFormat.h>`

## Data Fields
float | depth_m
float | soundVelocity_mPerSec
uint32_t | padding
float | temp_C
float | salinity

## Detailed Description

#SVP - Sound Velocity Profile. Data from one depth point contains information specified in this struct.

Definition at line 435 of file EMdgmFormat.h.

## Field Documentation

## ◆ depth_m

float depth_m

Depth at which measurement is taken. Unit m. Valid range from 0.00 m to 12000 m.

Definition at line 438 of file EMdgmFormat.h.

## ◆ soundVelocity_mPerSec

float soundVelocity_mPerSec

Measured sound velocity from profile. Unit m/s. For a CTD profile, this will be the calculated sound velocity.

Definition at line 439 of file EMdgmFormat.h.

## ◆ padding

uint32_t padding

Former absorption coefficient. Voided.

Definition at line 440 of file EMdgmFormat.h.

## ◆ temp_C

float temp_C

Water temperature at given depth. Unit Celsius. For a Sound velocity profile (S00), this will be set to 0.00.

Definition at line 441 of file EMdgmFormat.h.

## ◆ salinity

float salinity

Salinity of water at given depth. For a Sound velocity profile (S00), this will be set to 0.00.

Definition at line 442 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h