| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmIB_def Struct Reference

#IB - Results from online built in test (BIST). Definition used for three different BIST datagrams, i.e. #IBE (BIST Error report), #IBR (BIST reply) or #IBS (BIST short reply). More...

`#include <EMdgmFormat.h>`

Collaboration diagram for EMdgmIB_def:
[legend]

## Data Fields
EMdgmHeader | header
uint16_t | numBytesCmnPart
uint8_t | BISTInfo
uint8_t | BISTStyle
uint8_t | BISTNumber
int8_t | BISTStatus
uint8_t | BISTText

## Detailed Description

#IB - Results from online built in test (BIST). Definition used for three different BIST datagrams, i.e. #IBE (BIST Error report), #IBR (BIST reply) or #IBS (BIST short reply).

Definition at line 1372 of file EMdgmFormat.h.

## Field Documentation

## ◆ numBytesCmnPart

uint16_t numBytesCmnPart

Size in bytes of body part struct. Used for denoting size of rest of the datagram.

Definition at line 1376 of file EMdgmFormat.h.

## ◆ BISTInfo

uint8_t BISTInfo

0 = last subset of the message
1 = more messages to come

Definition at line 1377 of file EMdgmFormat.h.

## ◆ BISTStyle

uint8_t BISTStyle

0 = plain text
1 = use style sheet

Definition at line 1378 of file EMdgmFormat.h.

## ◆ BISTNumber

uint8_t BISTNumber

The BIST number executed.

Definition at line 1379 of file EMdgmFormat.h.

## ◆ BISTStatus

int8_t BISTStatus

0 = BIST executed with no errors
positive number = warning
negative number = error

Definition at line 1380 of file EMdgmFormat.h.

## ◆ BISTText

uint8_t BISTText

Result of the BIST. Starts with a synopsis of the result, followed by detailed descriptions.

Definition at line 1381 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h