| EM datagrams on *.kmall format Reg.no. 410224 rev C

- Main Page
- Related Pages
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
EMdgmSVPinfo_def Struct Reference

#SVP - Sound Velocity Profile. Info of size of structs, number of array entries etc. More...

`#include <EMdgmFormat.h>`

## Data Fields
uint16_t | numBytesInfoPart
uint16_t | numSamples
uint16_t | numBytesPerSVPpoint
uint16_t | numAbsCoeff
uint8_t | sensorFormat [4]
uint32_t | time_sec
double | latitude_deg
double | longitude_deg
float | freqAbsCoeff [MAX_NUM_ABSORPTION_COEFF]

## Detailed Description

#SVP - Sound Velocity Profile. Info of size of structs, number of array entries etc.

## Field Documentation

uint16_t numBytesInfoPart

Size in bytes of info struct. Used for denoting size current struct.

uint16_t numSamples

Number of sound velocity samples.

uint16_t numBytesPerSVPpoint

Size in bytes of EMdgmSVPpoint_def struct.

uint16_t numAbsCoeff

Number of absorption coefficient samples per depth.

uint8_t sensorFormat[4]

Sound velocity profile format:
'S00' = sound velocity profile
'S01' = CTD profile

uint32_t time_sec

Time extracted from the Sound Velocity Profile. Parameter is set to zero if not available.

double latitude_deg

Latitude in degrees. Negative if southern hemisphere. Position extracted from the Sound Velocity Profile. Parameter is set to define UNAVAILABLE_LATITUDE if not available.

double longitude_deg

Longitude in degrees. Negative if western hemisphere. Position extracted from the Sound Velocity Profile. Parameter is set to define UNAVAILABLE_LONGITUDE if not available.

float freqAbsCoeff[MAX_NUM_ABSORPTION_COEFF]

Frequencies for calculation of absorption coefficient. Actual number of frequencies in array is numAbsCoeff

The documentation for this struct was generated from the following file:

- EMdgmFormat.h