| EM datagrams on *.kmall format Reg.no. 410224 rev E

Data Fields
EMdgmSCLdataFromSensor_def Struct Reference

Part of clock datagram giving offsets and the raw input in text format. More...

`#include <EMdgmFormat.h>`

## Data Fields
float | offset_sec
int32_t | clockDevPU_nanosec
uint8_t | dataFromSensor [MAX_SCL_DATALENGTH]

## Detailed Description

Part of clock datagram giving offsets and the raw input in text format.

## Field Documentation

## ◆ offset_sec

float offset_sec

Offset in seconds from K-Controller operator input.

## ◆ clockDevPU_nanosec

int32_t clockDevPU_nanosec

Clock deviation from PU. Difference between time stamp at receive of sensor data and time in the clock source. Unit nanoseconds. Difference smaller than +/- 1 second if 1PPS is active and sync from ZDA.

## ◆ dataFromSensor

uint8_t dataFromSensor[MAX_SCL_DATALENGTH]

Clock data as received from sensor, in text format. Data are uncorrected for offsets.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h