| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmMRZ_extraSI_def Struct Reference

#MRZ - Extra seabed image samples. More...

`#include <EMdgmFormat.h>`

## Data Fields
uint16_t | portStartRange_samples
uint16_t | numPortSamples
int16_t | portSIsample_desidB [MAX_SIDESCAN_EXTRA_SAMP]
uint16_t | starbStartRange_samples
uint16_t | numStarbSamples
int16_t | starbSIsample_desidB [MAX_SIDESCAN_EXTRA_SAMP]

## Detailed Description

#MRZ - Extra seabed image samples.

Definition at line 1044 of file EMdgmFormat.h.

## Field Documentation

## ◆ portStartRange_samples

uint16_t portStartRange_samples

Start range of port side extra seabed image samples. Range in samples.

Definition at line 1047 of file EMdgmFormat.h.

## ◆ numPortSamples

uint16_t numPortSamples

Number of extra seabed image samples on port side.

Definition at line 1048 of file EMdgmFormat.h.

## ◆ portSIsample_desidB

int16_t portSIsample_desidB[MAX_SIDESCAN_EXTRA_SAMP]

Port side extra seabed image samples, as amplitudes in 0.1 dB.

Definition at line 1049 of file EMdgmFormat.h.

## ◆ starbStartRange_samples

uint16_t starbStartRange_samples

Start range of starboard side extra seabed image samples. Range in samples.

Definition at line 1050 of file EMdgmFormat.h.

## ◆ numStarbSamples

uint16_t numStarbSamples

Number of extra seabed image samples on starboard side.

Definition at line 1051 of file EMdgmFormat.h.

## ◆ starbSIsample_desidB

int16_t starbSIsample_desidB[MAX_SIDESCAN_EXTRA_SAMP]

Starboard side extra seabed image samples, as amplitudes in 0.1 dB.

Definition at line 1052 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h