| EM datagrams on *.kmall format Reg.no. 410224 rev C

- Main Page
- Related Pages
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
EMdgmMWCrxBeamData_def Struct Reference

#MWC - data block 2: receiver, specific info for each beam. More...

`#include <EMdgmFormat.h>`

## Data Fields
float | beamPointAngReVertical_deg
uint16_t | startRangeSampleNum
uint16_t | detectedRangeInSamples
uint16_t | beamTxSectorNum
uint16_t | numSampleData
int8_t * | sampleAmplitude05dB_p

## Detailed Description

#MWC - data block 2: receiver, specific info for each beam.

## Field Documentation

uint16_t detectedRangeInSamples

Two way range in samples. Approximation to calculated distance from tx to bottom detection [meters] = soundVelocity_mPerSec * detectedRangeInSamples / (sampleFreq_Hz * 2). The detected range is set to zero when the beam has no bottom detection

uint16_t numSampleData

Number of sample data for current beam. Also denoted Ns.

int8_t* sampleAmplitude05dB_p

Pointer to start of array with Water Column data. Lenght of array = numSampleData. Sample amplitudes in 0.5 dB resolution.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h