| EM datagrams on *.kmall format Reg.no. 410224 rev B

- Main Page
- Related Pages
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
EMdgmMWCtxInfo_def Struct Reference

#MWC - data block 1: transmit sectors, general info for all sectors More...

`#include <EMdgmFormat.h>`

## Data Fields
uint16_t | numBytesTxInfo
uint16_t | numTxSectors
uint16_t | numBytesPerTxSector
int16_t | padding
float | heave_m

## Detailed Description

#MWC - data block 1: transmit sectors, general info for all sectors

## Field Documentation

uint16_t numBytesTxInfo

Number of bytes in current struct.

uint16_t numTxSectors

Number of transmitting sectors (Ntx). Denotes the number of times the struct EMdgmMWCtxSectorData is repeated in the datagram.

uint16_t numBytesPerTxSector

Number of bytes in EMdgmMWCtxSectorData.

int16_t padding

Byte alignment.

float heave_m

Heave at vessel reference point, at time of ping, i.e. at midpoint of first tx pulse in rxfan.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h