| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmFCF_def Struct Reference

#FCF - Backscatter calibration file
The backscatter calibration file contains the measured backscatter offsets. These will be used to compensate for the default backscatter values. The datagram will contain the backscatter correction that is in use in the current line. More...

`#include <EMdgmFormat.h>`

Collaboration diagram for EMdgmFCF_def:
[legend]

## Data Fields
struct EMdgmHeader_def | header
struct EMdgmMpartition_def | partition
struct EMdgmFcommon_def | cmnPart
uint8_t | bsCalibrationFile [MAX_F_FILE_SIZE]

## Detailed Description

#FCF - Backscatter calibration file
The backscatter calibration file contains the measured backscatter offsets. These will be used to compensate for the default backscatter values. The datagram will contain the backscatter correction that is in use in the current line.

Definition at line 1300 of file EMdgmFormat.h.

## Field Documentation

## ◆ bsCalibrationFile

uint8_t bsCalibrationFile[MAX_F_FILE_SIZE]

Backscatter calibration file.

Definition at line 1306 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h