| EM datagrams on *.kmall format Reg.no. 410224 rev E

Data Fields
EMdgmMWCrxBeamPhase1_def Struct Reference

#MWC - Beam sample phase info, specific for each beam and water column sample. numBeams * numSampleData = (Nrx * Ns) entries. Only added to datagram if phaseFlag = 1. Total size of phase block is numSampleData * int8_t. More...

`#include <EMdgmFormat.h>`

## Data Fields
int8_t | rxBeamPhase

## Detailed Description

#MWC - Beam sample phase info, specific for each beam and water column sample. numBeams * numSampleData = (Nrx * Ns) entries. Only added to datagram if phaseFlag = 1. Total size of phase block is numSampleData * int8_t.

## Field Documentation

## ◆ rxBeamPhase

int8_t rxBeamPhase

Rx beam phase in 180/128 degree resolution.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h