| EM datagrams on *.kmall format Reg.no. 410224 rev C

- Main Page
- Related Pages
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
EMdgmIB_def Struct Reference

#IB - Results from online built in test (BIST). Definition used for three different BIST datagrams, i.e. #IBE (BIST Error report), #IBR (BIST reply) or #IBS (BIST short reply). More...

`#include <EMdgmFormat.h>`

Collaboration diagram for EMdgmIB_def:
[legend]

## Data Fields
EMdgmHeader | header
uint16_t | numBytesCmnPart
uint8_t | BISTInfo
uint8_t | BISTStyle
int8_t | BISTNumber
uint8_t | BISTStatus
uint8_t | BISTText

## Detailed Description

#IB - Results from online built in test (BIST). Definition used for three different BIST datagrams, i.e. #IBE (BIST Error report), #IBR (BIST reply) or #IBS (BIST short reply).

## Field Documentation

uint16_t numBytesCmnPart

Size in bytes of body part struct. Used for denoting size of rest of the datagram.

uint8_t BISTInfo

0 = last subset of the message
1 = more messages to come

uint8_t BISTStyle

0 = plain text
1 = use style sheet

int8_t BISTNumber

The BIST number executed.

uint8_t BISTStatus

0 = BIST executed with no errors
positive number = warning
negative number = error

uint8_t BISTText

Result of the BIST. Starts with a synopsis of the result, followed by detailed descriptions.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h