| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmSVTsample_def Struct Reference

#SVT - Sound Velocity at Transducer. Data sample. More...

`#include <EMdgmFormat.h>`

## Data Fields
uint32_t | time_sec
uint32_t | time_nanosec
float | soundVelocity_mPerSec
float | temp_C
float | pressure_Pa
float | salinity

## Detailed Description

#SVT - Sound Velocity at Transducer. Data sample.

Definition at line 533 of file EMdgmFormat.h.

## Field Documentation

## ◆ time_sec

uint32_t time_sec

Time in second. Epoch 1970-01-01. time_nanosec part to be added for more exact time.

Definition at line 535 of file EMdgmFormat.h.

## ◆ time_nanosec

uint32_t time_nanosec

Nano seconds remainder. time_nanosec part to be added to time_sec for more exact time.

Definition at line 536 of file EMdgmFormat.h.

## ◆ soundVelocity_mPerSec

float soundVelocity_mPerSec

Measured sound velocity from sound velocity probe. Unit m/s.

Definition at line 537 of file EMdgmFormat.h.

## ◆ temp_C

float temp_C

Water temperature from sound velocity probe. Unit Celsius.

Definition at line 538 of file EMdgmFormat.h.

## ◆ pressure_Pa

float pressure_Pa

Pressure. Unit Pascal.

Definition at line 539 of file EMdgmFormat.h.

## ◆ salinity

float salinity

Salinity of water. Measured in g salt/kg sea water

Definition at line 540 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h