| EM datagrams on *.kmall format Reg.no. 410224 rev D

- Main Page
- Related Pages
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
EMdgmSVTsample_def Struct Reference

#SVT - Sound Velocity at Transducer. Data sample. More...

`#include <EMdgmFormat.h>`

## Data Fields
uint32_t | time_sec
uint32_t | time_nanosec
float | soundVelocity_mPerSec
float | temp_C
float | pressure_Pa
float | salinity

## Detailed Description

#SVT - Sound Velocity at Transducer. Data sample.

## Field Documentation

uint32_t time_sec

Time in second. Epoch 1970-01-01. Ignoring leap second. time_nanosec part to be added for more exact time.

uint32_t time_nanosec

Nano seconds remainder. time_nanosec part to be added to time_sec for more exact time.

float soundVelocity_mPerSec

Measured sound velocity from sound velocity probe. Unit m/s.

float temp_C

Water temperature from sound velocity probe. Unit Celsius.

float pressure_Pa

Pressure. Unit Pascal.

float salinity

Salinity of water. Measured in g salt/kg sea water

The documentation for this struct was generated from the following file:

- EMdgmFormat.h