| EM datagrams on *.kmall format Reg.no. 410224 rev G

Data Fields
EMdgmMWCrxBeamPhase2_def Struct Reference

#MWC - Beam sample phase info, specific for each beam and water column sample. numBeams * numSampleData = (Nrx * Ns) entries. Only added to datagram if phaseFlag = 2. Total size of phase block is numSampleData * int16_t. More...

`#include <EMdgmFormat.h>`

## Data Fields
int16_t | rxBeamPhase

## Detailed Description

#MWC - Beam sample phase info, specific for each beam and water column sample. numBeams * numSampleData = (Nrx * Ns) entries. Only added to datagram if phaseFlag = 2. Total size of phase block is numSampleData * int16_t.

Definition at line 1166 of file EMdgmFormat.h.

## Field Documentation

## ◆ rxBeamPhase

int16_t rxBeamPhase

Rx beam phase in 0.01 degree resolution.

Definition at line 1168 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h