| EM datagrams on *.kmall format Reg. nr. 410224 rev I

Data Fields
EMdgmSPO_def Struct Reference

#SPO - Struct of position sensor datagram.
Data from active sensor will be motion corrected if indicated by operator. Motion correction is applied to latitude, longitude, speed, course and ellipsoidal height. More...

`#include <EMdgmFormat.h>`

Collaboration diagram for EMdgmSPO_def:
[legend]

## Data Fields
struct EMdgmHeader_def | header
struct EMdgmScommon_def | cmnPart
struct EMdgmSPOdataBlock_def | sensorData

## Detailed Description

#SPO - Struct of position sensor datagram.
Data from active sensor will be motion corrected if indicated by operator. Motion correction is applied to latitude, longitude, speed, course and ellipsoidal height.

Definition at line 221 of file EMdgmFormat.h.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h