| EM datagrams on *.kmall format Reg.no. 410224 rev E

Data Fields
EMdgmSHIdataFromSensor_def Struct Reference

Part of Height datagram, giving corrected and uncorrected data as received from sensor. More...

`#include <EMdgmFormat.h>`

## Data Fields
uint16_t | sensorType
float | heigthUsed_m
uint8_t | dataFromSensor [MAX_SHI_DATALENGTH]

## Detailed Description

Part of Height datagram, giving corrected and uncorrected data as received from sensor.

## Field Documentation

## ◆ heigthUsed_m

float heigthUsed_m

Height corrected using installation parameters, if any. Unit meter.

The documentation for this struct was generated from the following file:

- EMdgmFormat.h